| **Ahttp://en.termaheat.com/profiles/commerce_kickstart/themes/termaheat/images/icons/A.png[mm]** | **Bhttp://en.termaheat.com/profiles/commerce_kickstart/themes/termaheat/images/icons/B.png[mm]** | **C1[mm]** | **C2[mm]** | **C3[mm]** | **C4[mm]** | **75/65/20oC[W]** | **55/45/20oC[W]** | **http://en.termaheat.com/profiles/commerce_kickstart/themes/termaheat/images/icons/e%20I%20kl.png[W]** | **http://en.termaheat.com/profiles/commerce_kickstart/themes/termaheat/images/icons/e%20II%20kl.png[W]** | **D[mm]** | **E[mm]** | **F[mm]** | **http://en.termaheat.com/profiles/commerce_kickstart/themes/termaheat/images/icons/p.png[dm3]** | **http://en.termaheat.com/profiles/commerce_kickstart/themes/termaheat/images/icons/v.png[kg]** | **Product Code** |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| 1700 | 440 | 50 | 400 | 1660 | 440 | 529 | 277 | 600 | 500 | 300 | 1660 | 20 | 4.60 | 19.28 | WGINT170044 |
| 1700 | 540 | 50 | 500 | 1660 | 540 | 661 | 346 | 600 | 600 | 400 | 1660 | 20 | 5.73 | 22.54 | WGINT170054 |
| 1700 | 640 | 50 | 600 | 1660 | 640 | 925 | 485 | 1000 | 1000 | 500 | 1660 | 20 | 7.80 | 28.65 | WGINT170064 |
| 1900 | 440 | 50 | 400 | 1860 | 440 | 600 | 308 | 600 | 600 | 300 | 1860 | 20 | 5.06 | 21.37 | WGINT190044 |
| 1900 | 540 | 50 | 500 | 1860 | 540 | 762 | 392 | 800 | 800 | 400 | 1860 | 20 | 6.31 | 24.98 | WGINT190054 |
| 1900 | 640 | 50 | 600 | 1860 | 640 | 995 | 503 | 1000 | 1000 | 500 | 1860 | 20 | 8.60 | 31.79 | WGINT190064 |
| 1700 | 440 | 50 | 400 | 1660 | 440 | 370 | 193 | 400 | 400 | 300 | 1660 | 20 | 4.60 | 18.84 | WGINT170044 |
| 1700 | 540 | 50 | 500 | 1660 | 540 | 463 | 241 | 400 | 500 | 400 | 1660 | 20 | 5.73 | 21.99 | WGINT170054 |
| 1700 | 640 | 50 | 600 | 1660 | 640 | 648 | 337 | 600 | 600 | 500 | 1660 | 20 | 7.80 | 27.9 | WGINT170064 |

